{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Ark1","Ark2","Ark3"],"not_rendered":{"charts":0,"images":14,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Ark1","index":0,"n_rows":33,"n_cols":5,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Komponentliste  / Components list ",null,null,"HAKO 3000 - automatic machine       "]
["komponent","strømvejs#","TYPEbetegn","FORKLARING"]
["Component","page.col#","TYPEname","Explanation"]
["relay MSO","1.4D","Ermax 090 220 012","Master Switch Operated Standard AUTOrelay NO"]
["relay FUE","1.7D","Ermax 090 220 012","Fuel Enabled Standard AUTOrelay NO"]
["relay STE","1.8D","Ermax 090 220 012","Start Enabled Standard AUTOrelay NO"]
["relay USC","1.9D","Ermax 090 280 012","UnSafe Condition Standard AUTOrelay - NO/NC"]
["relay SRL","1.15D","Omron electronics MY4IN12DC(S)","Security ReLay 4X NO/NC"]
["relay AMB","1.6D","Ermax 090 280 012","Automatic Mode released Blink - Placed on rear side of main mounting plate"]
["relay AMO1","2.12D","Omron electronics G2R-1-T 12DC","Automatic Mode 1 - enable hydraulic steering for automatic control  - DANFOSS valve"]
["relay AMO2","3.1D","Omron electronics MY2IN12DC","Automatic Mode 2 - enable hydralic lift for automatic control  2X NO/NC"]
["relay RLU",null,"Ermax 090 280 012","activating Rear Lift UP"]
["relay RLD",null,"Ermax 090 280 012","activating Rear Lift DOWN"]
["relay EPT1","3.18D","Ermax 090 280 012","Enable PTO from ESX - overiding existing manual contact"]
["relay DA1","3.7D",null,"Disable Auxillary outputs when LIFT's are activated"]
["S1","2.17A","Telemecanique XS1 N08PA349","Engine speed - proximity sensor"]
["S2","2.19C","Telemecanique XS1 N08PA349","Prop Shaft speed - proximity sensor"]
["S3","2.16D","VISHAY SPECTROL 357-1-1-1S22-502","Special made position sensor - endless potentiometer and inhouse made amplifier"]
["S4","2.17D","VISHAY SPECTROL 357-1-1-1S22-502","Special made position sensor - endless potentiometer and inhouse made amplifier"]
[]
["P1","2.4C","5 Kohm LIN - SPECTROL 357-0-0-502","Potentiometer CVT"]
["P2","2.8C","5 Kohm LIN - SPECTROL 357-0-0-502","Potentiometer Engine Speed"]
["P3","2.","5 Kohm LIN - SPECTROL 357-0-0-502","Potentiometer Steering Angle"]
[]
["SB1","1.14C","Telemecanique XAL-K174F","Telemecanique - safety switch with red push bottun - ON REAR CORNER OF MACHINE "]
["SB2","1.14C","Telemecanique XAL-K174F","Telemecanique - safety switch with red push bottun - ON REAR CORNER OF MACHINE "]
["SB3","1.14C","Omron electronics A165EM02","Telemecanique - safety switch with red push bottun - IN REMOTE BOX"]
[]
["WB1","1.14B","Telemecanique XCK P106429 with XCK-T 06H29 ","Telemecanique - safety switch with wobble switch - "]
["WB2","1.14B","Telemecanique XCK P106429 with XCK-T 06H29 ","Telemecanique - safety switch with wobble switch - "]
[]
["CVTN","1.13A","Honeywell control system BZ - 2 RW - 822 - A 2 ","switch, with roler, to detect CVT is in neutral posistion"," "]
["                      Enviroment, Ressources and Technology, Agricultural Sciences, Faculty of Life, Copenhagen University. Højbakkegård Allé 9, DK-2630 Tåstrup - Denmark  ",null,null,null," "]

{"sheet":"Ark2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Ark3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}