# Static Call Graph for image .\Obj\STM3210E-EVAL.axf

#<CALLGRAPH># ARM Linker, RVCT3.1 [Build 939]: Last Updated: Sun May 24 08:07:44 2009

### Maximum Stack Usage = 0 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

### Mutually Recursive functions

- BusFaultException ⇒ BusFaultException
- HardFaultException ⇒ HardFaultException
- MemManageException ⇒ MemManageException
- UsageFaultException ⇒ UsageFaultException
- main ⇒ main

  ### Function Pointers

  - Reset_Handler
  - NMIException
  - HardFaultException
  - MemManageException
  - BusFaultException
  - UsageFaultException
  - SVCHandler
  - DebugMonitor
  - PendSVC
  - SysTickHandler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMA1_Channel1_IRQHandler
  - DMA1_Channel2_IRQHandler
  - DMA1_Channel3_IRQHandler
  - DMA1_Channel4_IRQHandler
  - DMA1_Channel5_IRQHandler
  - DMA1_Channel6_IRQHandler
  - DMA1_Channel7_IRQHandler
  - ADC1_2_IRQHandler
  - USB_HP_CAN_TX_IRQHandler
  - USB_LP_CAN_RX0_IRQHandler
  - CAN_RX1_IRQHandler
  - CAN_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - USBWakeUp_IRQHandler
  - TIM8_BRK_IRQHandler
  - TIM8_UP_IRQHandler
  - TIM8_TRG_COM_IRQHandler
  - TIM8_CC_IRQHandler
  - ADC3_IRQHandler
  - FSMC_IRQHandler
  - SDIO_IRQHandler
  - TIM5_IRQHandler
  - SPI3_IRQHandler
  - UART4_IRQHandler
  - UART5_IRQHandler
  - TIM6_IRQHandler
  - TIM7_IRQHandler
  - DMA2_Channel1_IRQHandler
  - DMA2_Channel2_IRQHandler
  - DMA2_Channel3_IRQHandler
  - DMA2_Channel4_5_IRQHandler
  - __main
  - main

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, entry.o($$startup$$))
  [Calls]

  - >> __init

  __call_main (Thumb, 2 bytes, Stack size 0 bytes, init.o(.emb_text))
  [Called By]

  - >> __init

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_vector.o(.text))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  __init (Thumb, 30 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __call_main
  [Called By]
  - >> __main

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  ADC1_2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC1_2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  ADC3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  BusFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFaultException))
  [Calls]

  - >> BusFaultException
  [Called By]
  - >> BusFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_RX1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_SCE_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel6_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel7_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel4_5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DebugMonitor (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMonitor))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI0_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI15_10_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI9_5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  FLASH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FLASH_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  FSMC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FSMC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  HardFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFaultException))
  [Calls]

  - >> HardFaultException
  [Called By]
  - >> HardFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_ER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_EV_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_ER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_EV_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  MemManageException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManageException))
  [Calls]

  - >> MemManageException
  [Called By]
  - >> MemManageException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  NMIException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMIException))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  PVD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PVD_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  PendSVC (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSVC))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RCC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RCC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTCAlarm_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SDIO_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SDIO_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SVCHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVCHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SysTickHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTickHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TAMPER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TAMPER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_BRK_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_CC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_TRG_COM_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_UP_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM6_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM7_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_BRK_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_CC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_TRG_COM_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_UP_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UART4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UART5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USBWakeUp_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_HP_CAN_TX_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_LP_CAN_RX0_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UsageFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFaultException))
  [Calls]

  - >> UsageFaultException
  [Called By]
  - >> UsageFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  WWDG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.WWDG_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 2 bytes, Stack size 0 bytes, main.o(i.main))
  [Calls]

  - >> main
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - init.o(.text)

  ### Local Symbols

  ### Undefined Global Symbols